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	Wisconsin Department of Agriculture, 
Trade and Consumer Protection
Division of Food and Recreational Safety
Bureau of Food and Recreational Businesses

	Supplemental Application for 
Direct Tanker Milking Operations
DATCP requires the installer, on behalf of the milk producer, to submit this supplemental application whenever a mobile tanker is used to store milk on the farm. Milk producers operating without a completed application are subject to enforcement action under Wis. Stat. ch. 97 and Wis. Admin. Code ch. ATCP 65.3. Personally identifiable information you provide may be used for purposes other than that for which it was collected. Wis. Stat. §15.04 (1)(m).

	Wis. Stat. § 97.22, Wis. Admin. Code § ATCP 65.14(6)

	INSTRUCTIONS
Complete all blanks applicable to this installation. This application must be accompanied by a detailed legible drawing of all the components pertaining to the Direct Ship. Use the numbers below and the numbers from the “Application for Milk Handling Equipment and Facility Construction” DFRS-BFRB-028 to identify all components.
Only plans that are complete and legible will be reviewed.
Coordinate the completion of this form between the installer, producer, milk hauler, and dairy plant to assure accurate information is provided.
Plan reviews are based on current Wisconsin regulations and standards.
Future modifications may be required as regulations and standards are updated.
PLEASE PRINT CLEARLY AND CHECK SPELLING



	26. Cooling Media Sample Port
	32. Sanitizing Station

	27. Tanker Valve Drip Pan
	33. Check Valve(s)

	28. Indicating Thermometer
	34. Milk Transfer Hose(s)

	29. Recording Thermometer Probe
	35. Drip Sampler

	30. Recording Device
	36. Milk Line Air Blow Fitting

	31. Tanker Dock Seal(s)
	37. Hard Surfaced Tanker Pad



	PRODUCER INFORMATION



	FIRM NAME:
     
	DATE:
     



	ADDRESS:
     



	CITY:
     
	STATE:
  
	ZIP CODE:
[bookmark: Text6]     




	PART I - EXTERIOR CONDITIONS

	Direct Tanker Equipment Installation (Check one)

	[bookmark: Check1]Tanker Parking Surface:   |_| Concrete   |_| Asphalt   |_| Other

	Extends Under Full Length of Tanker?   |_| Yes   |_| No (If No, explain below)

	[bookmark: Text1]     

	[bookmark: Check3][bookmark: Check4]Surface Sloped to Drain?   |_| Yes   |_| No   |_| Other - (Explain below)

	     

	Tanker Connection to Milkhouse:

	|_| Dock Seal   |_| Hose Port   |_| Enclosed Intake   |_| Other - (Explain below)

	     



	PART J - TANKERS(S)

	Direct Tanker Equipment Installation (Check one)

	Type of tanker used:   |_| Over the Road   |_| Hose Cabinet

	Who Owns the Milk Tanker(s)?   |_| Dairy Plant   |_| Producer   |_| Hauler

	Provide Milk Tanker Permit Numbers(s) below:



	[bookmark: Text2]     
	     

	     
	     

	     
	     



	Tanker(s) Meet 3A Sanitary Construction Standards?   |_| Yes   |_| No

	Tanker Modified to Fit Tight to Milkhouse?   |_| Yes   |_| No

	Tanker Access Ports Sealable?   |_| Yes   |_| No



	PART K - INTERMEDIATE COOLING

	Milk Cooling Method:   |_| Heat Exchanger   |_| Bulk Tank

	Provide all pertinent information in Section E of “Application for Milk Handling Equipment and Facility Construction” DFRS-BFRB-028

	Temperature Monitoring:   |_| Chart   |_| Electronic

	Enclose copy of the chart or chart specification.
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	PART L - FARM PROCEDURES

	[bookmark: Text3]How Many Milkings to Fill Tanker?      

	[bookmark: Text4]How Long Will Tanker Remain on Farm?       hrs.

	Where Is the Point of Sale for the Milk?   
|_| The Farm   |_| The Dairy Plant

	Is the Milking System Cleaned After Every Use?
|_| Yes   |_| No

	Transfer Hose, Check Valve, Exposed Interior Portion of Tanker Valve, Washed and Sanitized After Each Milking?   |_| Yes   |_| No

	Hoses and fittings of sanitary design for clean-in-place, no barbed fittings with hose clamps.


	Below is an example drawing of a Direct Ship operation added to an existing milking operation.

	[image: Drawing of a Direct Ship operation added to an existing milking operation.]



	PART M – WEIGHING AND SAMPLING OF THE MILK

	Performed by a Licensed Weigher and Sampler?
|_| Yes   |_| No

	Department Approved Facility for Receipt of Direct Ship Tankers?   |_| Yes   |_| No

	Milk Agitation Location:   
|_| Tanker   
|_| Storage/Silo - May not be commingled with other milk

	Method of Milk Agitation:
|_| Mechanical   |_| Air   |_| Other

	Location of Official Sampling:   |_| Farm   |_| Dairy Plant

	Type of Official Sampling:
|_| Tanker   |_| Storage Tank   |_| Drip Sampler

	[bookmark: Text5]Length of Agitation Prior To Sampling:       minutes

	Agitation protocol established in compliance with Standard Methods for the Examination of Dairy Products, Section 3.042 B. Test results on file at the receiving dairy plant.



MAIL this form in conjunction with the 
“Application for Milk Handling Equipment” (F-fd-31) to:
DATCP 
718 W Clairemont Ave, Suite 128
Eau Claire, WI  54701
OR         EMAIL both to: datcpdfsplanreview@wisconsin.gov
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