|  |
| --- |
| DFRS-BFRB-117.docx (rev. 03/2025) |
| Wisconsin Department of Agriculture, Trade and Consumer Protection*Division of Food and Recreational Safety*PO Box 8911, Madison, WI 53708-8911Phone: (608) 224-4720 Fax: (608) 224-4710 Email: datcpdfrsrec@wisconsin.gov |
| **VGBA Drain Cover Replacement Affidavit**  | *Wis. Admin. Code §§ ATCP 76.32(3) and 76.38* |
| Unless the operator has completed VGBA Drain and Equalizer Cover Replacement Log Form DFRS-BFRB-014 (rev 04/24), the operator shall record information about pool drain cover replacements here and certify that the instructions were followed for any drain cover stamped or otherwise identified as meeting 2017 VGBA standards, Consumer Product Safety Commission APSP-2016 2017. Failure to complete the form DFRS-BFRB-014 (rev 04/24) as required is subject to enforcement action under Wis. Stat. § 97.65 unless this form is completed and kept on file. Personally identifiable information you provide may be used for purposes other than that for which it was collected. (Wis. Stat. § 15.04 (1)(m)). |
| The operator shall maintain a copy of this report permanently.  |
| **PLEASE PRINT ALL INFORMATION. MAIL OR FAX REPORT TO THE ADDRESS LISTED AT THE TOP OF THE FORM.** |
| ESTABLISHMENT NAME:      | LICENSE NO FOR POOL:      |
| ESTABLISHMENT STREET ADDRESS:      | CITY:      | STATE:      | ZIP:      |
| LEGAL LICENSEE NAME: *(Name of sole proprietor, partnership, LLC, LLP, or Inc.)*      | CONTACT PERSON:      | PHONE:(     )-     -      |
| NAME / TYPE OF POOL OR WATER ATTRACTION:      |
| **DRAIN COVER REPLACEMENT INFORMATION** |
| BRAND AND MODEL NUMBER FOR REPLACEMENT:      | INSTALLATION DATE:      | GPM RATING:      | LOCATION (FLOOR OR WALL):      |
| CERTIFICATION: 2008 OR 2017 *(Look for stamp on cover or information in installation manual or Certificate of Conformity):*      |
| I certify that the drain cover(s) described above has/have been installed according to manufacturer instructions and that the gallons per minute rating is correct according to the Consumer Product Safety Commission APSP-2016 2017 VGBA standards. The gallons per minute rating of the drain cover(s) installed is/are higher than the highest peak flow of the pump. |
| SIGNATURE:       |
| PRINT NAME:       | PRINT DATE:       |